iv2299

Engine DXi11
GVW 19000 kg.
Gearbox mounted PTO
Front axle 7.5 t.
Sun visor
XPERT version heavy duty chassis

Flat bed:
Folding sides and tail gate
Twist locks
Hardwood floor
Bed size 630 x 250 cm
Side and tail gate height: 50 cm

**PM 14022 crane**
Horizontal Outreach: 8.45 m. Vertical Reach: 11.75 m.
Knuckle Boom Crane
Hour Meter
400 degrees slewing
Empty oil tank 88 l. capacity
High pressure filter mounted only in case of proportional valve block
pilot operated check valves on all cylinders
Plastic protection cover on valve block
Hook 7500 kg. capacity
Mounting kit
2 x stabilizer jacks
5 element valve block
Hydraulic wide outrigger booms - deviator 4 function - Span: 5500 mm
Overload protection device
Loading manometer
Hydraulic connection kit for 40 lt fix deliverying pump
Hydraulic piston pump - delivery 50 lt/1000 rpm
Cardan shaft