iv2299

Engine DXi11  
GVW 19000 kg.  
Gearbox mounted PTO  
Front axle 7.5 t.  
Sun visor  
XPERT version heavy duty chassis  
  
Flat bed:  
Folding sides and tail gate  
Twist locks  
Hardwood floor  
Bed size 630 x 250 cm  
Side and tail gate height: 50 cm  
  
**PM 14022 crane**  
Horizontal Outreach: 8.45 m. Vertical Reach: 11.75 m.  
Knuckle Boom Crane  
Hour Meter  
400 degrees slewing  
Empty oil tank 88 l. capacity  
High pressure filter mounted only in case of proportional valve block  
pilot operated check valves on all cylinders  
Plastic protection cover on valve block  
Hook 7500 kg. capacity  
Mounting kit  
2 x stabilizer jacks  
5 element valve block  
Hydraulic wide outrigger booms - deviator 4 function - Span: 5500 mm  
Overload protection device  
Loading manometer  
Hydraulic connection kit for 40 lt fix deliverying pump  
Hydraulic piston pump - delivery 50 lt/1000 rpm  
Cardan shaft